# Product description

* **Rapid removal of minor surface defects and swirl marks from all modern paint systems. Superb on darker colours**
* **Easy to remove fine sanding marks.**
* **High gloss and low dust technology.**
* **High lubrication system with longer polishing time.**
* **Low consumption and time saving formula.**
* **No aggressive smell & Easy to be wiped off.**

# Product Information

Available packages

|  |  |
| --- | --- |
| **Paste** | **Liquid** |
| **75 gm** | 125 Ml |
| **150 gm** | 300 Ml |
| **250 gm** | 1000 Ml |

**ml ml**

**ml ml**

**ml ml**

**Cutting range**

**Gloss range**

**ml ml**

**ml ml**

**ml ml**

# Key benefits

* **Reliable Cut Removes fine abrasive marks quickly and easily.**
* **Permanent finish contains no fillers so scratch marks won’t re- appear.**
* **High gloss system Excellent gloss .**
* **Silicone free 100% paintshop safe**
* **Swirl remover Swirl and holograms eliminated permenantly**
* **Can be used by machine with foam or lamb wool applicator as well as by hand**

# How To Use



**Spread at 1000 rpm and compound at 1500 – 2000 rpm**



ATTACH

**Soak the compounding foam in water.**

**Attach the pad to the polishing machine spin off the excess water.**

**Shake or mix the compound well, then apply to the pad or**

**Wipe clean with Finishing Cloth.**

**Soak the hand compounding foam or the microfiber cloth in water.**

**Shake or mix the compound well, then apply to microfiber cloth or surface.**

**Rub the product on the surface in back and forth motion**

**Apply water if necessary. Wipe clean with microfibe**